================================================================================
                                样例使用说明
                             Sample Description
================================================================================
功能描述：
此样例演示了sleep模式下，通过GPIO事件唤醒功能。

Function descriptions:
This sample demonstrates the sleep mode with GPIO event wake-up feature.
================================================================================
测试环境：
测试用板：PY32M070C_STK
MDK版本： 5.28
IAR版本： 9.20
GCC 版本：GNU Arm Embedded Toolchain 10.3-2021.10

Test environment:
Test board: PY32M070C_STK
MDK Version: 5.28
IAR Version: 9.20
GCC Version: GNU Arm Embedded Toolchain 10.3-2021.10
================================================================================
使用步骤：
1. 编译下载程序到MCU，并运行；
2. LED灯亮，按下按键，LED灯灭，串口打印"SLEEP MODE!"，进入sleep模式；
3. 在PA06上产生一个下降沿，程序退出sleep模式，并且串口打印"WAKEUP OK!"；
4. LED以200ms的间隔进行翻转。

Example execution steps:
1. Compile and download the program to the MCU and run it.
2. The LED is on, press the button, the LED turns off, and "SLEEP MODE!" is 
   printed on the serial port, entering the sleep mode.
3. Generate a falling edge on PA06 to wake up the program from sleep mode, and 
   "WAKEUP OK!" will be printed on the serial port.
4. The LED will toggle with an interval of 200ms.
================================================================================
注意事项：
STK板        USB转TTL模块
PA02(TX) --> RX
PA03(RX) --> TX
GND      --> GND

波特率:115200

1. 演示此样例功能时需要断开swd连接线并重新上电，因为默认情况下，仿真器会把
   DBGMCU_CR.DBG_STOP置位。
2. 注意关闭systick中断，防止该中断唤醒MCU。

Notes:
STK board        USB to TTL module
PA02(TX) --> RX
PA03(RX) --> TX
GND      --> GND

Baud rate: 115200

1. When demonstrating this sample, it is necessary to disconnect the SWD 
   connection and power on again because the debugger will set 
   DBGMCU_CR.DBG_STOP by default.
2. Pay attention to disable the systick interrupt to prevent it from waking 
   up the MCU.
================================================================================
